**Steering engine User Manual**

1. **Product features**

|  |  |
| --- | --- |
| **Model** | SG90 |
| **Torque** | 1.6kg/cm |
| **Speed of the reaction** | 0.1sec/60degree |
| **Action dead zone** | 10us |
| **Dead zone setting** | 5us |
| **Gear media** | nylon |
| **Working mode** | mock |
| **voltage** | 4.8V-5.0V |
| **size** | 23mm\*12.2mm\*29mm |
| **Fixed hole size** | 2.0mm |

1. **Interface definition**



